**LED Handrail Light for 24x24mm Groove with Beads (for Direct Clipping of the Light), Indoor / Outdoor, Symmetrical Light Distribution, Flexible LED Handrail Light** for Public Areas, Bridges, Railway Crossings, Underpasses, and Weather-, Exhaust-, and Vandalism-Prone Objects and Areas.

LED Handrail luminaire:

* Fully encapsulated LED light designed for use in handrail profiles with a groove 24x24mm with ribs for direct clipping into the handrail profile. No additional mounting is required.
* Together with the handrail profile, the light housing forms a cable channel (approx. 8x20mm) for wiring. The light is prepared for parallel connection.
* Light housing made of ABS plastic, with specially shaped reflector for wide symmetrical, continuous, even light distribution.
* Housing length: 206mm, 256mm, 306mm… (in 50mm increments) up to a maximum of 1506mm
* Light output: respective housing length minus 6mm
* Encapsulation material: clear PU
* Light distribution: symmetrical
* Operating voltage: 24VDC (20.5…26VDC)
* Protection class: IP69, Impact resistance class: IK10, vandal-proof, dimmable. Lifetime 50,000h
* Power: ............ (please enter – **6W/m, 10W/m or 20W/m (custom options available)**)
* Color temperature: ............ (please enter – **1800K, 2600K, 2900K, 3300K, 3500K, 4100K (custom options available)**)
* Suitable for direct clipping into curved LED handrail profiles ø42.4mm or 40x40mm, both with ribs. For a bending radius of at least 1.5m, no pre-bending of the light is required; it can be directly clipped in.

**Manufacturer: LUX GLENDER GmbH  
System: SAFE**